NPS LAB EXPERIMENT-6

Implementation of Smart home using Cisco packet tracer and verify the configuration.

Step 1: Open cisco packet tracer and drag and drop the following devices. Server PC Router Switch Fan Lamp Garage Speakers Connect the pc to the switch (F0/3), Server to switch (F0/1) Switch to the server (f2/1) and connect the router to the switch by the following wire in the picture.

Step 2: Click on each device (e.g., Smart Bulb). Goto the Config tab. Step 3: Select the Home Gateway as its network and assign the SSID (e.g., HomeNetwork).

Step 4: The devices can either receive an IP address dynamically (via DHCP) from the Home Gateway or you can manually assign static IPs under the Config > Wireless section

Step 5: Go to pc in that go to iot devices in that create username and password.

Step 6: Assign ip address to the pc and same address give in the fan in the remote server with username and password created in the iot device in the pc and repeat all the other devices like this.

Step 7: In the Desktop tab of the pc, go to IoT Monitor. Here you should see all the connected smart devices.

Step 8: You can control devices like turning on/off smart lights, locking/unlocking doors, etc

