NPS LABEXPERIMENT-3

Configuration of basic switch setup using Huawei/Cisco network switch.

Step 1: Open the Cisco packet tracer.

Step 2: Select three PC’S and one switch connect pc’s to switch through automatic cable wire.

Step 3: Double click on the pc and go to Desktop and in that click on ipconfig.

Step 4: Name the ip address of the each pc and click on 1 pc.

Step 5: Go to commandprompt in the desktop and type ping commandwith other ip address. And it replies from other pc’s.

Step 6: Save the file with a name





